**GLOSSARY**

The following terms shall have the respective meanings given below:

|  |  |
| --- | --- |
| **Abbreviation**  | **Description**  |
| ≥ | Larger than or equal to |
| ≤ | Smaller than or equal to |
| ± | Plus or minus |
| % | Percent |
| ℃ | Degree Celsius |
| AAMI | Association for the Advancement of Medical Instrumentation |
| ACGIH | American Conference of Governmental Industrial Hygienists |
| BI | Biological Indicators |
| BTU | British Thermal Unit |
| CISPR | Comité International Spécial des Perturbations Radioélectriques |
| CAN/CSA | Canada / Canadian Standard Association |
| CE | Conformité Européene |
| (D) | Depth |
| EC | European Commission |
| EMSD | Electrical and Mechanical Services Department |
| EN | European Norm |
| FDA | Food and Drug Administration |
| GB | Gigabyte |
| GUI | Graphical User Interface |
| (H) | Height |
| H2O2 | Hydrogen peroxide |
| Hz | Hertz |
| IEC | International Electrotechnical Commission |
| IMS | Independent Monitoring System |
| I/O | Input/ Output (network Lan port) |
| ISO | International Organization for Standardization |
| kg | Kilogram |
| (L) | Length |
| LCD | Liquid Crystal Display |
| mm | Millimetre |
| OSHA | Occupational and Safety Health Administration |
| ppm | Parts per million |
| PCD | Processing challenging device |
| RF | Radio frequency |
| USB | Universal Serial Bus |
| UV | Ultraviolet |
| (W) | Width |