**GLOSSARY**

The following terms shall have the respective meanings given below:

|  |  |
| --- | --- |
| **Abbreviation**  | **Description**  |
| ≤ | Smaller than or equal to |
| % | Percent |
| + | Plus |
| A | Amperes |
| A.C. | Alternating Current |
| APDs | Avalanche Photodiodes |
| APEOs | Alkylphenol Ethoxylates |
| BS | British Standards |
| CFC | Chlorofluorocarbons |
| CO2 | Carbon Dioxide |
| DICOM | Digital Imaging and Communications in Medicine |
| DIN | Deutsches Institut für Normung (meaning “German institute for standardization”) |
| EN | European Norm |
| GN | Gastronorm |
| HCFCs | Hydrochlorofluorocarbons |
| HP | Horsepower |
| Hz | Hertz |
| IP | Ingress Protection |
| IPX5 | IP – Ingress ProtectionX – not rated for particle protection like dust5 – protection from water projected from a nozzle |
| IPX6 | IP – Ingress ProtectionX – not rated for particle protection like dust6 – protection from strong jet of water |
| kg | Kilogram |
| kg/m2 | Kilogram per Square-meter |
| kW | Kilowatt |
| LCD | Liquid Crystal Display |
| mm | Millimeter |
| NPT | National Pipe Thread |
| RoHS | Restriction of Hazardous Substances |